**Emergency Operation System Examples**

1. Identify and install Oval Conference Room table (length 731.5cm, width 259.1cm, height 78.7cm) with the ability to recess or flip computer monitor, table seats 14

* Dell 9010 Small Form Factor Computers, 14ea
* Tray, Keyboard and Mouse, 14ea
* Samsung Sync Master 19” Monitor, 14ea
* Extron Cable Cubby 800, 3ea

1. Identify Executive Seating Conference Chairs, 16ea

* Conference Room Table, 14ea
* Office, 2ea

1. Identify Ergonomic Computer Chairs

* EOC Manager, 1ea
* Alternate EOC Manager, 1ea
* AV/IT Console
* Executive Administrative, 1ea
* Waiting Area, 4ea

1. Workstation w/Overhead Storage, 2ea in support of EOC Manager and Alternate

* Dell 9010 Small Form Factor Computers, 2ea
* Samsung Sync Master 24” Monitor, 2ea
* Printer Dell 2350dn (Network), 2ea
* Telephone, 2ea
* Copier/Printer, Canon 5045G

1. Audio Visual Console (L-Shape)

* Crestron Control Panel 12”
* Crestron AV 2 Processor
* QC Monitor 22” (wide screen)
* KVM Switch 4 Inputs/1 Output
* Dell 1910 Small Form Factor Computer w/Graphic Card, 4ea
* Wireless Keyboard and Mouse
* Telephone
* Laser Pointer - BTG-5 Focusable Green, 2ea
* Presenter Mouse - VP4450 Remote point Emerald Navigator
* Tandberg 1000MXP, 3ea
* Digital Sender, 2ea
* Fax Machine 5ea
* Flip Charts w/Paper & Markers, 6ea

1. Audio Visual Rack

* Side Panel and Top (Cherry Wood)
* Smoked Plexiglas Front Door
* Fan Kit (Rear Door), 2ea
* Blank Panels (Vented), 12 PC
* Lace Bars
* Casters (Four Wheel, Locking)
* Rack Screws

1. Workstation in support of Executive Assistance outside main door

* Dell 9010 Small Form Factor Computers, 2ea
* Samsung Sync Master 19” Monitor, 2ea
* Wireless Keyboard and Mouse
* Monitor 24”
* Copier/Printer, Canon 5045G
* Shredder DS18

1. Digital 4 Zone Clock
2. Cork Board (Large), 2ea
3. Panasonic Whiteboard w/Printer on roll around stand, 2ea
4. Smart Interactive 87” Whiteboard on Floor Stand
5. Curtain and curtain rod for office window purpose to eliminate sunlight entering conference room when camera is in use, video teleconference

**Audio Visual Equipment Examples**

1. Install multi-monitors display system (six 55” monitors) with multi-layer capability

* Samsung UE55A 55” Monitor, 7ea
* 55” Swing Six Monitors Wall Mount
* RGB Spectrum 4200 w/HDCP Option
* DVI to DVI 25ft Cable, 6ea
* DVI to DVI 50ft Cable, 8ea

1. Install router, Extron 12x8 to distribute signal through-out facility

* Tuner, 2ea
* AV Computer, 3ea
* Conference Room Table inputs (cable Cubby), 3ea
* HD Camera w/Wall Mount (outside main entrance)

1. Install video teleconference system, Cisco C40 (IP Only)

* Precision HD Camera
* Dual Screen capability
* Multi-Site capability
* 12 Advance Care Program

1. Install audio conference system

* ClearOne Converge 1212A
* Overhead Speakers, 6ea
* Gooseneck microphones, 12ea with individual mute and un-mute capability
* ClearOne Max Attach (4 Pods)

**Office AV System Examples**

Install AV system

* Samsung 42’ Monitor with Tuner, 2ea
* Extron 192, display local computer, 2ea
* Printer Dell 2350dn (Network), 2ea
* Telephone, 2ea
* GN 2125 Headset with adapter cables, 2ea
* Digital Camera

**Information Technology Examples**

Expand network infrastructure to accommodate additional computers, printers and VTC system

* Cisco 48 Port Switch
* IT Rack (Secure Door w/Key)
* Rack Screws, 100ea
* Cable CAT 6a, 2000ft
* Crimp Tool, 2ea
* Connector RJ45, 200ea
* Dell 9010 Small Form Factor Computers, 12ea

**Building Facility Examples**

1. Modify existing floor to allow for cable distribution

* Remove existing tile floor, dig, burier and install conduit, 6ea allowing for Power and LAN cables to be routed where needed and eliminating existing trip hazards.

1. Back-Up Power

* Identify and install individual Standby Uninterruptible Power System in support of EOC and Admin area

1. Air Conditioning System

* Identify and install Air Conditioning Duct System

1. Lights (Relook lighting system in Facility)

* Install separate circuit for EOC Facility and Office lighting
* Install dimmer light fluorescent ballast and dimmer switch

1. Cell Phone Signal Weak

* Install cell phone repeater, see list of service provider below

1. Zain jo
2. Umniah
3. Orange
4. Wall in need of painting, color to be selected at a later date

* Paint entire facility
* Replace all cover plates (Electrical Outlet and Jacks, Local Area Network)

Conduct pilot test with three external site’s (Governance) selected by Ministry of Health, outfit site’s with equipment listed below.

* Computer (Dell 9010 Small Form Factor), 2ea
* Keyboard & Mouse, 2ea
* Monitor 19”, 2ea
* Printer, 2ea
* Telephone, 2ea
* Fax Machine, 2ea
* Tandberg 1000MXP, 1ea